For these two mounts only:

mount-sherpa-mini-r1-rapido-hf-2.2.stl
mount-sherpa-mini-r1-volcano-dragon-2.2.stl

Please be aware that the PTFE tube should be 2 mm shorter for these two mounts than the rest as the mount has a slimmer mounting plate for the extruder. 

The reason for this is that the Sherpa Mini is a bit taller than the other supported extruders and with these tall hotends (Rapido and Volcano Dragon), the top of the extruder could hit the frame of the printer.